Transmissivity Calibration Targets for Twin Cities Metropolitan Area Groundwater-Flow Model V3.0
This page last updated: 03/26/2014
Metadata created using Minnesota Geographic Metadata Guidelines

Go to Section:
1. Overview
2. Data Quality
3. Data Organization
4. Coordinate System
5. Attributes
6. Distribution - Get Data
7. Metadata Reference

Section 1 | Overview
Originator | Barr Engineering Company
Title | Transmissivity Calibration Targets for Twin Cities Metropolitan Area Groundwater-Flow Model V3.0
Abstract | This dataset contains transmissivity calibration targets used for the Twin Cities Metropolitan Area Groundwater-Flow Model Version 3.0
Purpose | This dataset was developed for a regional groundwater flow model for the Twin Cities Metropolitan Area
Time Period of Content Date | 03/26/2014
Currentness Reference | This data reflects data based on model calibration completed in 2013.
Progress | Complete
Maintenance and Update Frequency | As needed
Spatial Extent of Data | This data covers the extent of the Twin Cities metropolitan area groundwater flow model version 3.
Bounding Coordinates | -94.626 -94.678 45.941 44.096
Place Keywords | Twin Cities, Anoka County, Carver County, Chisago County, Dakota County, Hennepin County, Isanti County, Ramsey County, Scott County, Sherburne County, Washington County, Wright County
Theme Keywords | transmissivity, groundwater
Theme Keyword Thesaurus | None
Access Constraints | None
Use Constraints | None
Contact Person Information | Lanya Ross, Principal Environmental Scientist, Water Supply Planning Metropolitan Council 390 Robert Street North St. Paul, MN 55101-1805 Phone: 651-602-1803 Fax: 651-602-1130 Email: Lanya.Ross@metc.state.mn.us
Browse Graphic | None available
Associated Data Sets |
Section 2 | Data Quality
Attribute Accuracy | There are no known deficiencies.
Logical Consistency | There are no known deficiencies
Completeness | This data reflects data from model calibration complete in 2013.
Horizontal Positional Accuracy |
Lineage | Transmissivity values were obtained from pumping test results compiled by Tipping (2011)
Section 3 | Spatial Data Organization (not used in this metadata)
Section 4 | Coordinate System
Horizontal Coordinate Scheme | Universal Transverse Mercator
UTM Zone Number | 15
Horizontal Datum | NAD83
Horizontal Units | meters
Section 5 | Attributes
Overview | Unique: Minnesota County Well Index Unique ID WellName: Well Name from CWI utme: UTM NAD83 Zone 15 N Easting utmn: UTM NAD83 Zone 15 N Northing Aquifer: Aquifer for test. Aquifer codes are: Ku = Cretaceous Os = St. Peter Sandstone Op = Prairie du Chien Group Cj = Jordan Sandstone Csl = St. Lawrence Formation Ctc = Tunnel City Group Cw = Wonewoc Sandstone Ce = Eau Clairie Formation Cms = Mt. Simon-Hinckley Sandstones T_Measured: Measured transmissivity in square meters per day T_Model: Model transmissivity in square meters per day
Detailed Citation | None
Table Detail: |

Section 6 | Distribution
Publisher |
Publication Date | 03/26/2014
Contact Person Information | Lanya Ross, Principal Environmental Scientist, Water Supply Planning Metropolitan Council 390 Robert Street North St. Paul, MN 55101-1805 Phone: 651-602-1803 Fax: 651-602-1130 Email: Lanya.Ross@metc.state.mn.us
Distributor's Data Set Identifier |
Distribution Liability |
Ordering Instructions |
Online Linkage | None available
Section 7 | Metadata Reference
Metadata Date | 03/26/2014
Contact Person Information | Lanya Ross, Principal Environmental Scientist, Water Supply Planning Metropolitan Council 390 Robert Street North St. Paul, MN 55101-1805 Phone: 651-602-1803 Fax: 651-602-1130 Email: Lanya.Ross@metc.state.mn.us
Metadata Standard Name | Minnesota Geographic Metadata Guidelines
Metadata Standard Version | 1.2
Metadata Standard Online Linkage | http://www.lmic.state.mn.us/gc/stds/metadata.htm

This page last updated: 03/26/2014
Go back to top